Decontamination Process

At the start of the day


1. Prior to first use of the day, the washer disinfector / EDW must have undergone a self-disinfection cycle. This process may be automated of pre-set to occur at a designated time dependent on make of EDW. Complete daily  checks for EDW's in line with manufacturer's instructions plus CFPP01-06.
2. Disinfect irrigation pumps for flushing of endoscopes during cleaning.
3. For morning lists, process scopes and valves or remove scopes from the drying cabinets (if available on site).
4. Any scopes processed are checked for leaks, damage or faults.
5. Manually clean and process scopes through EDW ready for use on list. The EDW will perform the task of high level disinfection on all parts of the internal and external channels of the endoscope. A completed cycle with print out will confirm that the process has been successful.
6. Remove the endoscope and valves from the EDW and place into the hard based tray with a green liner and traceability form or store in the drying cabinet.



Between Cases


After the last case


Follow steps 4, 5 and 6 as per start of the day
7.  Scopes will be stored overnight in the drying cabinets.
8. Or in an appropriate ventilated cupboard for re-processing scopes at the start of the day.
9. Decontaminate irrigation pumps.


Lumen Endoscopes
As per start of the day, follow points 4, 5, and 6.













